# Copy to /etc/conf.d/wan-snapshot on each host (optional).
# Source from cron:  . /etc/conf.d/wan-snapshot 2>/dev/null; /usr/local/bin/wan-snapshot.sh

# --- Raspberry Pi (external / home vantage) ---
# WAN_SNAPSHOT_ROLE=pi
# WAN_SNAPSHOT_LOG=/var/log/wan-quality.log
# ROUTER_PING_TARGET=10.7.6.228
# FE_PING_TARGET=10.7.0.10
# BE_PING_TARGET=10.7.16.128

# --- Gentoo FE ---
# WAN_SNAPSHOT_ROLE=fe
# WAN_SNAPSHOT_LOG=/var/log/wan-quality.log
# FE_PING_TARGET=10.7.0.10
# BE_PING_TARGET=10.7.16.128
# ROUTER_PING_TARGET=10.7.6.228

# --- Debian edge router (monstro) ---
# WAN_SNAPSHOT_ROLE=router
# WAN_SNAPSHOT_LOG=/var/log/wan-quality.log
# FE_PING_TARGET=10.7.0.10
# BE_PING_TARGET=10.7.16.128

# Shared
# WAN_SNAPSHOT_EXTRAS=1
# PING_COUNT=10
# PING_DEADLINE_S=15
